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CERTIFICATE OF ANALYSIS
CERTIFIED REFERENCE MATERIAL

TURBIDITY STANDARD SOLUTION 1000 NTU

Certificate No.                                    NICPCRM00250526/01
Product ID			CRM0025
Lot No 				NICP20052601
Description			Turbidity Standard 1000 NTU
Mfg. Date			May 2026
Shelf-life		December 2027
Storage Condition		Below 8°C
Composition	Hexamethylene Tetramine, Hydrazine Sulphate & Reagent Grade I Water

	Measurand
	Units 
	Certified Value
	Expanded Uncertainty (k = 2)


	Turbidity Standard Solution

	NTU
	999.3
	± 17.42


[bookmark: _Hlk218260521]Measurement Method	Testing was performed by an ISO/IEC 17025:2017 accredited testing laboratory. Characterization, homogeneity, and stability of the CRM were established in accordance with ISO 33405:2024. The assigned value and Measurement uncertainty was evaluated in accordance with ISO 13528:2022.
Metrological Traceability	Measurement results are metrologically traceable to SI units via an unbroken chain of calibration and comparison, using Certified Reference Materials traceable to national or international reference standards.
Intended Use                   	It is intended to use for calibration standard & validation of Nephelometric method 
Packaging 	100 mL of Turbidity standard solution is filled in a white HDPE bottle, which is then sealed and packed in a polyester (PE) zipper pouch.
Instructions for handling	Shake well before use and never pipette directly from the Bottle.
The internal pressure of the Bottle may be slightly different from the atmospheric pressure at the user’s location. Open slowly and carefully to avoid dispersion of the material.
Health and safety Information	All certified reference material (CRM) should be used only by qualified laboratory personnel. Please refer to the safety data sheet for detailed information about the nature of any hazard and appropriate precautions to be taken.
Accreditation 	NICP is accredited by the National Accreditation Board for Testing and Calibration Laboratories (NABL) in accordance with ISO 17034:2016 and ISO/IEC 17025:2017.
Application	This Certified Reference Material is intended for use as a calibration standard for Turbidity measurement using analytical test procedures, and for verification of analytical equipment and test methods.
Correct use	The solution bottle should be open for the minimum time required to dispense the solution.
Information		This certificate related solely to the lot no. given above.
The CRM was gravimetrically prepared using precision analytical balances calibrated and verified by an ISO/IEC 17025:2017 accredited calibration laboratory.
Certificate issue date:	1/06/2026                                           
Certificate Version:		NICP20012026
 					
Certificate Issued By
                                                                                                                                      Mr. Prakash Dubey
   Authorized Signatory NICP
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